**FloSet®*105***

**Specification Text**

**PN25 rated, forged DZR FloSet® 105, with nickel-plated CW617N brass drain, suitable for heating and cooling applications with water temperatures from -15°C to 115°C.**

**Assembly to include the FlowCon 5-position flushing by-pass with extended handles incl. full isolation, on 105mm centres, FlowCon Strainer (optional) with integrated Test Points and line-size Drain in the Flow Branch, FlowCon Green Pressure Independent Control Valve suitable for medium to high flow rates and FlowCon flow venturi metering station for medium to high flow rates with integrated Test Points in the return branch; FlowCon self-calibrating full stroke IP54-rated Electric Actuator, either modulating or raise lower.**

**Valve assembly must be supplied labelled with the correct terminal unit reference, duty, flow rate, insert ID, setting, metering station ID & signal and QR code link to technical documentation.**