**FloSet®*80***

**Specification Text ABV Assembly**

**PN20 rated, forged DZR FloSet® 80, suitable for heating and cooling applications with water temperatures from 0°C to 110°C.**

**Assembly to include the FlowCon 5-position flushing by-pass with extended handles incl. full isolation, on 80mm centres; FlowCon flow venturi metering station for extra low to high flow rates and FlowCon IVC strainer in the flow branch; FlowCon E-Just or Composite Automatic Balancing Valve suitable for low flow rates from 0.008 l/s in the return branch, flushing, drain & test points in the flow and return branches.**

**Valve assembly must be supplied labelled with the correct terminal unit reference, duty, flow rate, insert ID, setting, metering station ID & signal and QR code link to technical documentation.**