**FloSet®*Kit***

**PN16 rated, forged DZR FloSet® Kit, suitable for heating and cooling applications with water temperatures from 0C to 120C.**

**First Fit Kit to include the FlowCon 5-position flushing by-pass with extended handles incl. full isolation, on 80mm centres; FlowCon flow venturi metering station for extra low to high flow rates in the return branch and FlowCon IVC strainer (optional) in the flow branch.**

**FCU Kit to include a FlowCon Green Pressure Independent Control Valve suitable for low flow rates from 0.005 l/s in the return branch, flushing, drain & test points in the flow and return branches and FlowCon self-calibrating full stroke IP54-rated Electric Actuator, either modulating or raise lower.**

**Kits must be supplied labelled with the correct terminal unit reference, duty, flow rate, insert ID, setting, metering station ID & signal and QR code link to technical documentation.**