**FloSet®*Smart***

**Specification Text**

**PN25 rated, forged DZR FloSet® Smart, suitable for heating and cooling applications with water temperatures from -10°C to 120°C.**

**Handed to suit duty. Vertical or horizontal alignment. Assembly to include the FlowCon 5-position flushing by-pass incl. full isolation, on 40mm centres. FlowCon flow venturi metering station for extra low to high flow rates and FlowCon Strainer option in the Flow Branch. Belimo EPIV with MP-Bus BACnet actuator and flow sensors in the return branch. Flushing, drain & test points in the flow and return branches.**

**Valve assembly must be supplied labelled with the correct terminal unit reference, duty, flow rate, Control Valve ID, setting, metering station ID & signal and QR code link to technical documentation.**